;
; 2d HPGL configuration file 
;
; NOTE: there are no z moves output
;
; History
; Who When     What
; === ======== ========================================95
; bem 25/09/00 Written
;
DESCRIPTION = "2D HPGL (*.plt)"
;
FILE_EXTENSION = "plt"
;
; Set units used in file - MM
;
UNITS = mm
;
; Cariage return - line feed at end of each line ?
; END_OF_LINE = "[13][10]"
;
; Set up default formating for variables
;
; Each step is 0.025mm
;
;
FORMAT = [X|@||1.0|40]
FORMAT = [Y|@||1.0|40]
FORMAT = [Z|@||1.0|40]
; Home tool positions 
FORMAT = [XH|@||1.0|40]
FORMAT = [YH|@||1.0|40]
FORMAT = [ZH|@||1.0|40]
;
; Set up program header
;
; initialise program start
START = "IN;"
;
;
; Set home position (pen-up)
START = "PU;PA;"
;
; Select tool (pen) 1
START = "SP1;"
;
;
; Program moves
;
PLUNGE_RATE_MOVE = ""
RETRACT_MOVE = ""
FIRST_RAPID_RATE_MOVE = "PU;PA[X],[Y];"
RAPID_RATE_MOVE  = "PA[X],[Y];"
;
FIRST_FEED_RATE_MOVE = "PD;PA[X],[Y];"
FEED_RATE_MOVE   = "PA[X],[Y];"
;
; End of file
END = "PU;"
;
END = "SP0;"


