;
; G - Code configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; Hector Henry/Jen Van Gaalen  	March/2003 Written
; TLS Altered for Routech Xilog MMI March/2004 
; GJM ALtered for Quality Woodworking April 2004
;
DESCRIPTION = "Routech Xilog MMI (inch) (*.xxl)"
;
FILE_EXTENSION = "xxl"
;
UNITS = INCH
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
;
; Set up default formating for variables
;
; Rapid Feed Rate
FORMAT = [FR|#|V=|1.1|25.4]
; Feed Rate
FORMAT = [FC|#|V=|1.0|25.4]
; Plunge Feed Rate
FORMAT = [FP|#|V=|1.0|25.4]
; Tool moves in x,y and z
FORMAT = [X|#|X=|1.3]
FORMAT = [Y|#|Y=|1.3]
FORMAT = [Z|#|Z=|1.3]
FORMAT = [IA|@|I=|1.3]
FORMAT = [JA|@|J=|1.3]
; Tool Format
FORMAT = [T|@|T=|1.0|1.0]
; Spindle 
FORMAT = [S|@|S=|1.0]
; Safe Z 
FORMAT = [SZ|@|D=|1.2]
;
; Header Format
;
START = "H DX=[XMAX] DY=[YMAX] DZ=[ZMATERIAL] -A C=0 T=0 R=1 *IN /DEF"
TOOLCHANGE = ""
;
; Program moves
;
RAPID_RATE_MOVE        = "XG0 [X] [Y] [Z] [FR] [S] [SZ] [T]"
FIRST_FEED_RATE_MOVE   = "G1 [X] [Y] [Z] [FC]"
FEED_RATE_MOVE         = "G1 [X] [Y] [Z]"
;
PLUNGE_RATE_MOVE       = "G1 [X] [Y] [Z] [FP]"
;
;
; Circular Interpolation Moves
;
FIRST_CW_ARC_MOVE      = "G2 [X] [Y] [Z] [IA] [JA] [FC]"
CW_ARC_MOVE            = "G2 [X] [Y] [Z] [IA] [JA]"
;
FIRST_CCW_ARC_MOVE     = "G3 [X] [Y] [Z] [IA] [JA] [FC]"
CCW_ARC_MOVE           = "G3 [X] [Y] [Z] [IA] [JA]"
;
END = "XN X=0 Y=0 V=45 F=1"
END = "XN T=101"
