;
; Techno-Isel configuration file 
;
; History
;
; Who When     What
; === ======== ========================================
; TM 10/02/97  Written for Hankook Delcam
; bem 21/03/00 Added DESCRIPTION and FILE_EXTENSION fields
;
DESCRIPTION = "Techno-Isel (*.tap)"
;
FILE_EXTENSION = "tap"
;
UNITS = MM
;
; Cariage return - line feed at end of each line
;
END_OF_LINE = "[13][10]"
;
;
; Block numbering 
;
LINE_NUM_START      = 0
LINE_NUM_INCREMENT  = 1
LINE_NUM_MAXIMUM    = 99999
LINE_NUM_INC_ON_USE = 1
;
; Set up default formating for variables
;
; Line numbering
FORMAT = [N|@||06.0]
; Spindle Speed
FORMAT = [S|@|S|1.0]
; Feed Rate
FORMAT = [F|#|F|1.0|0.006]
; Tool moves in x,y and z
FORMAT = [X|@|X|03.0|100]
FORMAT = [Y|@|Y|03.0|100]
FORMAT = [Z|@|Z|03.0|100]
;
; Home tool positions 
FORMAT = [XH|@|X|03.0|100]
FORMAT = [YH|@|Y|03.0|100]
FORMAT = [ZH|@|Z|03.0|100]
;
; Set up program header
;
START = "[N] 1MF_PBL V1.0"
START = "[N] ************************"
START = "[N] Type: ArtCAM cutterpath"
START = "[N] Created: ??"
START = "[N] ************************"
START = "[N] INITTOOL"
START = "[N] SPINDLE RPM0"
START = "[N] COOLANT OFF"
START = "[N] GETTOOL 0"
START = "[N] VEL 0"
START = "[N] SPINDLE RPM[S]"
START = "[N] FASTABS [ZH]"
START = "[N] FASTABS [XH] [YH]"
;
RAPID_RATE_MOVE        = "[N] FASTABS [X] [Y] [Z]"
FIRST_FEED_RATE_MOVE   = "[N] @ [X] [Y] [Z]"
FEED_RATE_MOVE         = "[N] @ [X] [Y] [Z]"
;
; Program moves
;
; FEED_RATE_MOVE = "[N] MOVEABS [X] [Y] [Z]"
;
; End of file
END = "[N] FASTABS [X] [Y] [Z]"
END = "[N] FASTABS [X] [Y]"
END = "[N] SPINDLE RPM0"
END = "[N] COOLANT OFF"
END = "[N] PROGEND"




