;; DS2490.inf

;; *********  PLEASE READ ***********
;; The wizard cannot create exact INF files for all buses and device types. 
;; You may have to make changes to this file in order to get your device to
;; install. In particular, hardware IDs and logical configurations require
;; intervention.

[Version]
Signature="$CHICAGO$"
Class = 1Wire
ClassGuid = {C49068C2-B65C-4de2-83D9-D4B945AA5C91}
provider=%ProviderName%


;[SourceDisksNames]
;1 = "",,,
 
;[SourceDisksFiles]
;DS2490.sys = 1
;DS2490api.dll = 1
;DS2490comm.dll = 1

[DestinationDirs]
DS2490.Files.Drv.NT = 10, System32\Drivers
;DS2490.Files.Dll.NT = 10, System32


[Manufacturer]
%MfgName% = DS2490_model

[DS2490_model]
%DeviceDesc% = DS2490.Device.Install, USB\VID_04FA&PID_2490




; --- Windows'2000 install ---

[DS2490.Device.Install.NT]
DriverVer = 11/02/2000
CopyFiles=DS2490.Files.Drv.NT	;, DS2490.Files.Dll.NT
AddrReg = DS2490.AddReg.NT


[DS2490.Device.Install.NT.Services]
Addservice = DS2490, 0x00000002, DS2490.AddService

[DS2490.Files.Drv.NT]
DS2490.sys

;[DS2490.Files.Dll.NT]
;DS2490api.dll
;DS2490comm.dll

[ClassInstall32.NTx86]
AddReg = 1WireClass.AddReg.NT

[1WireClass.Addreg.NT]
HKR,,,,"1Wire Devices" ; device-class friendly name 
HKR,,Icon,,1
;[HKR,,SilentInstall,,1]
;[HKR,,NoInstallClass,,1]
;[HKR,,NoDisplayClass,,1]


[DS2490.AddService]
DisplayName    = %SvcDesc%
Description    = %DeviceDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_AUTO_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\DS2490.sys


;---------------------------------------------------------------;

[Strings]
ProviderName="Dallas Semiconductor"
MfgName="Dallas Semiconductor"
DeviceDesc="USB Host for 1-Wire Microlan"
SvcDesc="DS2490 (USB Host for 1-Wire Microlan)"




