5. Print

5.1. Print Function

This printer can achieve the following print functions:

Functions | Diagram
Manual Duplex |
Collate |
Reverse Print |
N-in-1 |
Poster Printing (Only for Windows system) |
Zoom Print |
Custom Size |

| Note: | • You can select the 2x2 Poster printing in N-in-1 to realize the poster printing function. • You can open the Printing Preferences and click the Help button to view the specific function explanation. For information about how to open the help document, see Section 5.2.

5.2. Opening Help Document

Open the Printing Preferences and click the Help button (Only for Windows system) .

The Help document contains the User Guide for the printer.

5.3. Manual Duplex

1. The printer driver supports manual duplex.

| Note: | • If the paper is thin, it may wrinkle. • If the paper is curled, make it flat and put it back into the manual feeder tray. • If the manual duplex function causes a paper jam, see Section 9.1 for instructions.

2. Ensure that a certain amount of paper is loaded into the automatic feeder tray before printing.

| Note: | • For loading paper, see Section 2.2. • For the type of media that can be printed with the automatic feeder tray, see Chapter 10.5. It is recommended to use the standard paper. • Some paper media are not suitable for duplex printing. Trying duplex printing may damage the printer. When Paper Type is Thick or Transparency, please do not try duplex printing. If 2 x 2 Poster printing is checked in the Printing Preferences dialog box, Manual Duplex will not be supported. • If the paper loaded into the automatic feeder tray exceeds 150 pages, paper will jam or will not be fed in.

3. The printing steps are as follows (Only for Windows system) :

a) Open the document to be printed from the application (such as Notepad), and select Print from the File menu.

b) Select Pantum Printer.

c) Click Printing Preferences or Properties button for the settings of print.

d) Check Manual Duplex in the Basic tab and click OK after completing the settings.

e) Click Print.

| Note: | • It is recommended to raise the output tray to prevent the paper from sliding out of it. If you choose not to raise the output tray, we recommend that you immediately remove the printed paper output from the printer.

f) A window of Duplex Recovery Tips will automatically pop up to inform you of the specific operation procedures.

g) Remove the printed paper from the output tray, tidy the paper and put it back into the automatic feeder tray print-side (blank side) facing up.

| Note: | • Remove a stack of paper from the output tray and put them into the automatic feeder tray after flipping the up and down sides. Do not change the order of the stack of paper during this process.

h) Press OK on the control panel to continue printing.

The printer will print all the even pages on the other side of the paper in turn.

5.4. Cancel Job

Press the Cancel button on the control panel to cancel the job you want to cancel during the printing process.