10. Product Specification

10.1. Overview

Functions | PC monochrome printing, PC colored/monochrome scanning, monochrome copying
Memory | 128 MB
Interface Type | USB 2.0 (High-speed interface)
Supported Operating Systems | Microsoft Windows Server 2003/Server 2008/ Server 2012/XP/Vista/Win7/Win8 (32bit&64bit) Mac OS X 10.5/10.6/10.7/10.8
LCD Display | 16 English characters × 2 lines
Power Supply | 220V Model: AC220~240V(-15%,+10%), 50/60Hz(±2Hz), 3A; 110V Model: AC110~127V(±10%),50/60Hz(±2Hz), 6A (Note: For the power supply and voltage that is suitable for this printer, please refer to the nameplate on the back of the printer.)
Noise | Printing | ≤54db
Stand-by | ≤35db
Power Consumption | Print | Average 450W Max. Power 660W (25°C)
Stand-by | 50 W
Sleep | ≤3.5 W
TEC① | ≤ 1.45kwh
Operation Environment | Operation temperature range (best print quality): 5-35(10-32)°C Operation humidity range: 20~80% RH
Product Size (W*D*H) mm | 399*327*299
Weight (Excluding Toner Cartridge) | About 8kg

| Note: | ① Typical Energy Consumption (TEC): Refers to the weekly energy consumption of a product in kilowatt-hour (kWh) obtained by the test method and the calculation method stipulated by the relevant technical specifications.

10.2. Scanning Specification

Scan Source | Platen
Optical System | CIS
Scan Driver | TWAIN WIA
Scan Resolution | Optics 1200*1200DPI
Maximum Scan Size (Tablet) | 216 mm x 297 mm
Bit Depth | 24 bit/8 bit/1 bit
Output Function | Scan to PC

10.3. Printing Specification

Print Speed | A4: 16ppm, 20ppm LTR: 16ppm, 21ppm
Print Language | GDI
Resolution | 1200*600DPI
Max Monthly Volume | 20,000 pages

10.4. Copying Specification

Copy Speed | A4: 16ppm, 20ppm LTR: 16ppm, 21ppm
Resolution | 1200*600DPI
Continuous Copying Pages | 1-99
Copying Mode | Text, image, text + image
Special Copy Function | One-click ID Copy, Receipt Copy and N-in-1 copy

10.5. Paper Handling Capacity

Media Type | Plain, thick, special paper (cardstock, label, envelope, etc.)
Media Size | A4, A5, JIS B5, IS0 B5, A6, Letter, Legal, Executive, Folio, Oficio, Statement, Japanese Postcard, Monarch Env, DL Env, C5 Env, C6 Env, No.10 Env, ZL, Big 16K, Big 32K, 16K, 32K, B6
Media Weight | Automatic feed: 60~105g/m², manual feed: 60~163g/m²
Paper Input Capacity | Standard: 150 pages (80g/m²), manual: 1 page
Paper Output Capacity | 100 pages